**Coatings & Applications**

****

|  |  |
| --- | --- |
| **Yellow Bare Swab (YBS)** | **Yellow Criss Cross (YCC) & Yellow Long Coat (YLG-B)** |
| Drying and wiping (1.61 KM) | Long distance wiping (4.83 KM) |
| Coated both ends for Bi-Directional | Light cleaning |
| Bullet nose available for multi-diameter lines | Light scraping |
| Handling ropes, cables or chains | Max compression |
| Sealing pig | Bullet nose available for multi-diameter lines |
| Gauging pipe I.D. | Handling ropes, cables or chains |
| Line proving |  |
| Pigging multi-diameter lines |  |
| **Stock sizes available: ¾” O.D. up to 48-1/2” O.D. in ½” increments. Other sizes can be ordered upon request.** | |

|  |  |
| --- | --- |
| **Red Bare Squeegee (RBS)** | **Red Bare Squeegee Fully Coated (RBS F/C)** |
| Regular drying (16 KM) | Regular wiping (16 KM) |
| Bullet nose or bi-directional | Bullet nose or bi-directional |
| Handling ropes, cables or chains available | Handling ropes, cables or chains available |
| Bare poly foam with coating on back end for sealing | Can be made with cavity for tracking |
| Dewatering | Poly coating seals the entire pig |
| Gauging pipe I.D. | Resistant to harsh chemicals (H2S, CO2, Diesel Mix) |
| Line proving | Can be used for batching instead of solid cast urethane |
| Soft product removal in any pipe | Remains flexible with coating application for maneuvering bends |
| **Sizes available: ½” O.D. up to 30” O.D. Bigger sizes available only in bi-directional option.** | |

|  |  |
| --- | --- |
| **Red Criss Cross (RCC)** | **Red Criss Cross Wire Brush & Plastic Brush (RCCWB) & (RCCPB)** |
| Longer distance wiping & cleaning (16 KM) | Longer distance scraping & cleaning (16 KM) |
| Bullet nose or bi-directional | Bullet nose or bi-directional |
| Handling ropes, cables or chains available | Handling ropes, cables or chains available |
| More wear resistance | Removal of slag, lime build-up and rust & corrosion |
| Removal of paraffin and/or condensate | Removal of paraffin, scale & hardened build-up |
| Thick and/or soft internal deposits | Best used for scraping steel pipe |
| More abrasive in plastic pipe | Plastic wire brush is also available-no scaring or damage to pipe walls & reduced static during pigging |
| **Sizes available: ½” O.D. up to 30” O.D. Bigger sizes available only in bi-directional option.** | |

|  |  |
| --- | --- |
| **Red Bare Squeegee with Mesh (RBS ME)** | **RBS with Ceramic Bead or Silicon Carbide (Sil C) Grit** |
| Plastic mesh molded into foam for strength | Used for applications where internal deposits are hardened from heat |
| Extra-long mileage compared to RBS (25 KM) | Sil C is very abrasive – consult is recommended |
| Used for PVC, fiberglass, poly, epoxy-lined pipe & steel pipe | Ceramic Bead makes for a very hard coating, but has a smooth finish mainly for polishing |
| Both coatings are recommended for heavier densities such as 8lb., 10lb. & harder | |
| Sil C and Ceramic Bead and all other coating applications can be applied to balls (excluding mesh), RBS, SBD, Double Dish, foam pushers and more. | |
| Other additives can be introduced for strength & speed; please consult within. | |
| **Sizes available: ½” O.D. up to 30” O.D. Bigger sizes available only in bi-directional option.** | |