## BALLS & PUSHERS

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | **Pipeline Pigging Specialties Ltd. manufactures a**  **wide range of Pig Balls & Pushers**  **Various urethane durometers, foam densities, colors,**  **numbers, solid cast urethane, foam core urethane,**  **solid foam, swab core foam**  **fully coated, criss cross coated, wire coated**  X:\PIG Pics\Website Pics\Sil C Balls - Web.JPGX:\PIG Pics\Product 1 - RBS Balls.JPGX:\PIG Pics\Product 1 - Ure Balls.JPG**and so much more…** | | | | | | | | | | | | |
| **3/4”** | | **1”** | **2”** | **3”** | **4”** | **5”** | **6”** | **7”** | **8”** | **9”** | **10”** | **12”** | **16”** |
| **7/8”** | | **1-1/8”** | **2-1/8”** | **3-1/8”** | **4-1/8”** | **5-1/4”** | **6-1/4”** | **7-1/4”** | **8-1/4”** | **9-1/4”** | **10-1/4”** | **12-1/4”** |  |
|  | | **1-1/4”** | **2-1/4”** | **3-1/4”** | **4-1/4”** | **5-1/2”** | **6-1/2”** | **7-1/2”** | **8-1/2”** | **9-1/2”** | **10-1/2”** |  | **24”** |
|  | | **1-3/8”** | **2-1/2”** | **3-3/8”** | **4-3/8”** | **5-3/4”** |  |  | **8-3/4”** |  |  |  |  |
|  | | **1-1/2”** | **2-5/8”** | **3-1/2”** | **4-1/2”** |  |  |  |  |  |  |  | **30”** |
|  | | **1-5/8”** | **2-3/4”** | **3-3/4”** | **4-3/4”** |  |  |  |  |  |  |  |  |
|  | | **1-3/4”** | **2-7/8”** | **3-7/8”** | **4-7/8”** |  |  |  |  |  |  |  |  |