|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| STYLE | TYPE | | DENSITY | FUNCTION |
| SSD | **SBD** (Scarlet Bare Durafoam) | | 8 LBS./CU.FT. | Heavy Drying Up to 200 MI (321 KM) |
| SCC | **SCC** (Scarlet Criss Cross) | | 8 LBS./CU.FT. | Heavy Wiping Up to 200 MI (321 KM) |
| SCC-WB | **SCCWB** (Scarlet Criss Cross Wire Brush) | | 8 LBS./CU.FT. | Heavy Scraping Up to 200 MI (321 KM) |
| SCC-SC | **SCC-SC** (Scarlet Criss Cross Silicon Carbide) | | 8 LBS./CU.FT. | Heavy Scraping Up to 200 MI (321 KM) |
| SCC-T | **SCC-T** (Turning) | | 8 LBS./CU.FT. | Heavy Wiping Up to 300 MI (482 KM) |
| SCC-WB-T | **SCC-WB-T** (Turning) | | 8 LBS./CU.FT. | Heaviest Scraping Up to 300 MI (482 KM) |
| SCC-SC-T | **SCC-SC-T** (Turning) | | 8 LBS./CU.FT. | Heaviest Scraping Up to 300 MI (482 KM) |
| RBS | **RBS** (Red Bare Squeegee) | | 5 LBS./CU.FT. | Regular Drying  Up to 10 MI (16 KM) |
| RCC | **RCC** (Red Criss Cross) | | 5 LBS./CU.FT. | Regular Wiping Up to 10 MI (16 KM) |
| RCC-WB | **RCCWB** (Red Criss Cross Wire Brush) | | 5 LBS./CU.FT. | Regular Scraping Up to 10 MI (16 KM) |
| RCC-SC | **RCC-SC** (Red Criss Cross Silicon Carbide) | | 5 LBS./CU.FT. | Regular Scraping Up to 10 MI (16 KM) |
| RCC-T | **RCC-T** (Turning) | | 5 LBS./CU.FT. | Longer Wiping Up to 25 MI (40 KM) |
| RCC-WB-T | **RCC-WB-T** (Turning) | | 5 LBS./CU.FT. | Longer Scraping Up to 25 MI (40 KM) |
| RCC-SC-T | **RCC-SC-T** (Turning) | | 5 LBS./CU.FT. | Longer Scraping Up to 25 MI (40 KM) |
| YBS | **YBS** (Yellow Bare Swab) | | 2 LBS./CU.FT. | Light Drying Up to 1 MI (1.61 KM) |
| YCC | **YCC** (Yellow Criss Cross) | | 2 LBS./CU.FT. | Light Drying Up to 1 MI (1.61 KM) |
| YCC-SC | **YCC-SC** (Yellow Criss Cross Silicon Carbide) | | 2 LBS./CU.FT. | Light Drying Up to 1 MI (1.61 KM) |
| YBS-B | **YBS-B** (Bullet) | | 2 LBS./CU.FT. | Light Drying Up to 1 MI (1.61 KM) |
| YCC-T | **YCC-T** (Turning) | | 2 LBS./CU.FT. | Light Drying Up to 3 MI (4.83 KM) |
| YCC-SC-T | **YCC-SC-T** (Turning) | | 2 LBS./CU.FT. | Light Drying Up to 3 MI (4.83 KM) |
| SPECIAL APPLICATIONS | | | | |
| Maxi-Brush | | **Power Brush** | 8 LBS./CU.FT. | Maximum Scraping |
| Maxi-Brush-Lightwire | | **Power Brush Light Wire** | 20 LBS./CU.FT. | Long Range Cleaning Up to 500 MI (804 KM) |

**Pipeline Pigging Specialties Ltd.**

**603-21 Ave**

**Nisku, Alberta, Canada T9E 7X9**

**780-955-7776**

[**www.pipelinepigging.ca**](http://www.pipelinepigging.ca)[**info@pipelinepigging.ca**](mailto:info@pipelinepigging.ca)